**HOROLOGICAL MACHINE N°10 ‘BULLDOG’**

The relationship between man and watch is as nuanced as the one between man and dog. The best examples of such connections last for years, even decades, shaping lives and stories. In some cases, the watch chooses its owner as much as the other way around. After all, whether it’s your first or hundredth time, there’s something special about the moment you set eyes on The One. So it is, as they say, with Man’s Best Friend. Presenting Horological Machine N°10 ‘Bulldog’.

A rounded, compact body of titanium, red gold or microblasted stainless steel with black PVD coating coupled with a generous ration of sapphire crystal. Two prominent aluminium time-display “eyes”, rolling at anyone who dares look its way. A collar studded with projections that allow you to wind the mainspring or set the time. Stout but flexible “legs” that wrap firmly around your wrist. A massive jaw. And above all, a big heart beating steadily at 2.5Hz (18,000bph).

Just like the creature for which it is named, there’s more to HM10 Bulldog than meets the eye. Its hinged jaws open and shut according to the amount of wind left in its mainspring — a fully closed mouth tells you that “Bulldog” is wound down and ready for a nap. If you can clearly see the rows of shining teeth lining the jaws, get ready, because that means “Bulldog” is full of fight, charged up with a 45 hours of mainspring energy. This massive power-reserve indication has been carefully designed and calibrated to consume the least energy possible, allowing HM10 Bulldog to direct its considerable mainspring torque solely towards its suspended balance and its revolving hour and minute domes.

The manual-winding engine of HM10 Bulldog was designed and developed in-house, leveraging the best of MB&F’s technical expertise built up over the years; longtime members of the MB&F Tribe will recognise elements that hew closely to the horological lab’s best-loved creations. The large suspended balance that hovers just beneath the central dome of sapphire crystal was made possible by the various iterations of this mechanism in the Legacy Machine collection. The massive jaws that indicate the level of mainspring wind are a much-expanded demonstration of the power-reserve management that was first deployed in the 2014 LM1 Xia Hang. The paper-thin aluminium domes have their roots in the HM3 Frog and were refined in 2014’s HM6. Even the grillework design motif in the “ribs” set beneath the balance and in the tail-end of the body echoes the automotive-inspired HM8, HMX and HM5. Taken altogether, the message is clear: HM10 Bulldog is a highly bred machine.

Despite its outsize personality — measuring 45mm across, 54mm from nose to tail and with a maximum height of 24mm — HM10 Bulldog is surprisingly wearable. Its sprung strap attachment “legs” allow the body to fit closely around the wrist, with the calf-leather strap as robust as any well-made leash — fastened with either a folding buckle or Velcro system. HM10 Bulldog is assembled with highly distilled expertise in micro-mechanical engineering. Fitting the requisite elements of timekeeping and time display within such a limited three-dimensional volume, while maintaining top levels of artistry and finish, requires careful balance between technical and aesthetic factors.

MB&F creations have always attracted a highly loyal audience and HM10 Bulldog returns the favour in spades: its allegiances go solely to its owner. Both the time indication and the power reserve display are visible only from the point of view of the wearer.

One final piece of advice for those who come across Horological Machine N°10 ‘Bulldog’ is engraved on its body, like a cautionary message you might find on the collar of a particularly feisty canine. The beast may be intimidating, but it ultimately exists in service of another. People would do well to remember — “Forget the dog, beware of the owner”.

MB&F Horological Machine N°10 ‘Bulldog’ is available in two launch editions: grade 5 titanium body with blue “eyes”, and 18K red-gold and titanium body with black “eyes”.

In 2022, HM10 Bulldog adds ‘Dark Bulldog’ versions in three colors to the collection, limited to 8 pieces each:

* Stainless steel with black PVD coating and black eyes
* Stainless steel with black PVD coating and blue eyes
* Stainless steel with black PVD coating and red eyes

**INSPIRATIONS FOR HM10 BULLDOG**

The design came to Maximilian Büsser while he was travelling in Japan; Horological Machine N°10 ‘Bulldog’ bounded up in his mind’s eye just as a loyal pup might greet a returning master.

*“What you see now in front of you is more or less exactly what I saw at the time,”* says Büsser, *“and it was the first time I actually saw a watch in my mind, just like that.”*

HM10 Bulldog coalesced from various MB&F influences and motifs that dedicated enthusiasts of the brand will immediately recognise. In a deeply affirmative way, HM10 Bulldog is simultaneously a reflection of MB&F and a paean to the fidelity of their followers. The traditional saying “as stubborn as a bulldog” parallels the determination of MB&F to chart an untraditional path outside of conventional watch design, sometimes with creations that have polarised the horological community. In similar vein, the British bulldog may be a dog of pedigree and stature, but it is certainly no crowd-pleaser.

The Latin root for the word “animal” is *anima*, meaning “soul” or “spirit”; the enlivening element. Little wonder that the MB&F creations that draw inspiration from the natural world — such as Horological Machine N°3 ‘Frog’ and Horological Machine N°7 ‘Aquapod’ — have also provoked some of the strongest responses. HM10 Bulldog follows this evocative path, with its large eyes, expressively mobile mouth and exposed heart.

**MORE ABOUT THE HM10 ENGINE**

The mechanics driving Horological Machine N°10 ‘Bulldog’ are entirely new but deeply familiar. Completely designed and developed in-house, the HM10 engine is the technical confluence of the various areas of movement expertise at MB&F, honed over years of experience.

The eye-catching balance, suspended beneath the central sapphire crystal dome and beating at the traditional cadence of 2.5Hz (18,000bph), first appeared in an MB&F creation in 2011, with the debut of Legacy Machine N°1. Since then, this technically challenging mechanism has become a unique icon of MB&F, appearing in the majority of Legacy Machines, Horological Machine N°9, and now HM10 Bulldog.

Powerful and startling, the revolving time-telling domes of HM10 Bulldog originated in the conical hour- and minute-modules of the first Horological Machine N°3, the creation that cemented MB&F’s reputation as a disruptive horological force. Subsequently, the cones took on rounded forms in HM3 ‘Frog’, but the one factor that remained constant was the urgent need to make them as light as possible, so that they placed minimal stress on the rest of the engine. Conventional milling processes were reworked and tolerances were sliced micro-fine in order to produce paper-thin aluminium components in three dimensions. These components later appeared again in Horological Machine N°6, this time paired with conical gearing to enable the highly precise display of time.

The 301-component HM10 engine is manual-winding, with a single barrel that imparts 45 hours of power reserve, indicated by the opening and shutting of external hinged jaws. Whereas conventional examples of power-reserve display will aim for a simple hand indicator that consumes as little energy as possible, HM10 Bulldog has chosen to make a statement of strength with its impossible-to-miss display. Separate crowns are actuated for winding and time-setting, located towards the rear of the HM10 Bulldog body.

**HM10 BULLDOG**

**TECHNICAL SPECIFICATIONS**

**Horological Machine N°10 ‘Bulldog’ is available in five versions:**

**- Ti version: grade 5 titanium case with blue hour and minute domes;**

**- RT version: 18K red gold and titanium case with black hour and minute domes;**

**- ‘Dark Bulldog’ versions: case in microblasted stainless steel with black PVD coating with black, blue or red hour and minute domes. Limited editions of 8 pieces each.**

**Engine**

Manual-winding in-house movement.

Bespoke flying 14mm balance wheel with four traditional regulating screws floating above the domed dials.

Super-LumiNova on the hour and minute domes and markers.

Single barrel with 45 hours of power reserve.

Frequency: 18,000bph / 2.5Hz.

Number of components: 301.

Number of jewels: 34.

Left crown at 11 o'clock for winding; right crown at 1 o'clock for setting the time.

**Functions/indications**

Hours on left dome (aluminium dome rotating in 12 hours).

Minutes on right dome (aluminium dome rotating in 60 minutes).

Power reserve indicated in 3D by the opening and closing of the jaws (end of power reserve = closed jaws).

**Case**

Ti version: grade 5 titanium.

RT version: 18K 5N+ red gold and grade 5 titanium.

‘Dark Bulldog’ versions: microblasted stainless steel with black PVD coating.

Dimensions: 54mm x 45mm x 24mm.

Water resistant to 5ATM / 50m / 160’.

**Sapphire crystals**

2 sapphire crystals treated with anti-reflective coating on both sides.

**Strap & buckle**

RT version: hand-stitched brown calf-leather strap with custom-designed red gold folding buckle.

Ti version: hand-stitched blue calf-leather strap with Velcro system and titanium buckle.

‘Dark Bulldog’ versions: hand-stitched black calf-leather strap with Velcro system and titanium buckle.

**‘FRIENDS’ RESPONSIBLE FOR HM10 BULLDOG**

**Concept**: Maximilian Büsser / MB&F

**Design**: Eric Giroud / Through the Looking Glass

**Technical and production management**: Serge Kriknoff / MB&F

**R&D**: Simon Brette, Ruben Martinez, Thomas Lorenzato and Joey Miserez / MB&F

**Case:** Riccardo Pescante / Les Artisans Boîtiers

**Sapphire crystals:** Sylvain Stoller / Novo Crystal

**Anti-refection treatment for sapphire crystals:** Anthony Schwab / Econorm

**Precision turning of wheels, pinions and axes:** Paul André Tendon / Bandi, Jean-François Mojon / Chronode, Daniel Gumy / Decobar Swiss, Atokalpa and Le Temps Retrouvé

**Springs and jumper:** Alain Pellet / Elefil Swiss

**Balance wheel:** Laurent Matthey / Precision Engineering

**Balance spring:** Stefan Schwab / Schwab-Feller

**Barrel:** Daniel Gumy / Decobar Swiss

**Plates, bridges and indexes:** Benjamin Signoud / Amecap, Marc Bolis / 2B8

**Hand-finishing of movement components:** Jacques-Adrien Rochat and Denis Garcia / C.-L. Rochat

Hand-engraving of movement: Glypto

**PVD-treatement:** Pierre-Albert Steinmann / Positive Coating

**Buckle:** Mecalex

**Crowns:** Cheval Frères

**Dials (hours and minutes domes):** Hassan Chaïba and Virginie Duval / Les Ateliers d’Hermès Horlogers

**Movement assemblage:** Didier Dumas, Georges Veisy, Anne Guiter, Emmanuel Maitre, Henri Porteboeuf and Mathieu Lecoultre / MB&F

**In-house machining:** Alain Lemarchand, Jean-Baptiste Prétot and Romain Camplo / MB&F

**Quality control:** Cyril Fallet / MB&F

**After-Sales Service:** Thomas Imberti / MB&F

**Strap:** Multicuirs

**Presentation box:** Olivier Berthon / Soixanteetonze

**Logistics and production:** David Lamy, Ashley Moussier, Fanny Boutier and Houda Fayroud / MB&F

**Marketing & Communication:** Charris Yadigaroglou, Vanessa André, Arnaud Légeret and Camille Reix / MB&F

**M.A.D.Gallery:**Hervé Estienne / MB&F

**Sales:** Thibault Verdonckt, Virginie Marchon, Cédric Roussel and Jean-Marc Bories / MB&F

**Graphic design:** Sidonie Bays / MB&F

**Product photography:** Maarten van der Ende, Alex Teuscher and Laurent-Xavier Moulin

**Portrait photography:** Régis Golay / Federal, Alex Teuscher

**Website:** Stéphane Balet / Idéative

**Film:** Marc-André Deschoux / MAD LUX and RJ41

**Texts:** Suzanne Wong / WorldTempus

**MB&F – GENESIS OF A CONCEPT LABORATORY**

Founded in 2005, MB&F is the world’s first-ever horological concept laboratory. With almost 20 remarkable calibres forming the base of the critically acclaimed Horological and Legacy Machines, MB&F is continuing to follow Founder and Creative Director Maximilian Büsser’s vision of creating 3-D kinetic art by deconstructing traditional watchmaking.

After 15 years managing prestigious watch brands, Maximilian Büsser resigned from his Managing Director position at Harry Winston in 2005 to create MB&F – Maximilian Büsser & Friends. MB&F is an artistic and micro-engineering laboratory dedicated to designing and crafting small series of radical concept watches by bringing together talented horological professionals that Büsser both respects and enjoys working with.

In 2007, MB&F unveiled its first Horological Machine, HM1. HM1’s sculptured, three-dimensional case and beautifully finished engine (movement) set the standard for the idiosyncratic Horological Machines that have followed – all Machines that tell the time, rather than Machines to tell the time. The Horological Machines have explored space (HM2, HM3, HM6), the sky (HM4, HM9), the road (HM5, HMX, HM8) and the animal kingdom (HM7, HM10).

In 2011, MB&F launched its round-cased Legacy Machine collection. These more classical pieces – classical for MB&F, that is – pay tribute to nineteenth-century watchmaking excellence by reinterpreting complications from the great horological innovators of yesteryear to create contemporary objets d'art. LM1 and LM2 were followed by LM101, the first MB&F Machine to feature a movement developed entirely in-house. LM Perpetual, LM Split Escapement and LM Thunderdome broadened the collection further. 2019 marked a turning point with the creation of the first MB&F Machine dedicated to women: LM FlyingT; and MB&F celebrated 10 years of Legacy Machines in 2021 with the LMX. MB&F generally alternates between launching contemporary, resolutely unconventional Horological Machines and historically inspired Legacy Machines.

As the F stands for Friends, it was only natural for MB&F to develop collaborations with artists, watchmakers, designers and manufacturers they admire.

This brought about two new categories: Performance Art and Co-creations. While Performance Art pieces are MB&F machines revisited by external creative talent, Co-creations are not wristwatches but other types of machines, engineered and crafted by unique Swiss Manufactures from MB&F ideas and designs. Many of these Co-creations, such as the clocks created with L’Epée 1839, tell the time while collaborations with Reuge and Caran d’Ache generated other forms of mechanical art.

To give all these machines an appropriate platform, Büsser had the idea of placing them in an art gallery alongside various forms of mechanical art created by other artists, rather than in a traditional storefront. This brought about the creation of the first MB&F M.A.D.Gallery (M.A.D. stands for Mechanical Art Devices) in Geneva, which would later be followed by M.A.D.Galleries in Taipei, Dubai and Hong Kong.

There have been distinguished accolades reminding us of the innovative nature of MB&F’s journey so far. ‘To name a few, there have been no less than 7 awards from the famous Grand Prix d'Horlogerie de Genève: in 2021, MB&F received two prizes: one for LMX as the Best Men’s Complication and one for the LM SE Eddy Jaquet ‘Around The World in Eighty Days’ in the ‘Artistic Crafts’ category, in 2019, the prize for Best Ladies Complication went to the LM FlyingT, in 2016, LM Perpetual won the Best Calendar Watch award; in 2012, Legacy Machine No.1 was awarded both the Public Prize (voted for by horology fans) and the Best Men’s Watch Prize (voted for by the professional jury).In 2010, MB&F won Best Concept and Design Watch for the HM4 Thunderbolt. In 2015 MB&F received a Red Dot: Best of the Best award – the top prize at the international Red Dot Awards – for the HM6 Space Pirate.